V10.16: Unsteady Under and Over

(Related to Textbook Section 10.6.4 - Underflow Gates)

In an open channel water can flow under an object such as a sluice gate and over an object such as a weir.

The flow shown here simulates the sudden release of water under an object as may happen from a break in a dam. The water flows into a quiescent layer of fluid and sloshes back-and-for over a weir. The results are from a physics-based animation derived from a computational fluid dynamics (CFD) simulation for this particular flow geometry (see Appendix A for details about CFD).
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