	

Exploration & Production
	DATA SHEET
	N°      

	
	Project:
	     

	
	DS EP PVV 142
Rev. 00 – 01/2011
	Data Sheet for Manual Operated Ball Valve



	

Exploration & Production
	DATA SHEET
	[bookmark: DSNUM]N°      

	
	Project:
	[bookmark: PROJECT]     

	
	DS EP PVV 142
Rev. 00 – 01/2011 
	Data Sheet for Manual Operated Ball Valve



	Rev. Date
	[bookmark: date]     
	[bookmark: Texte31]     
	[bookmark: Texte35]     
	[bookmark: Texte39]     
	[bookmark: Texte43]     
	[bookmark: Texte47]     

	Written
	[bookmark: Texte28]     
	[bookmark: Texte32]     
	[bookmark: Texte36]     
	[bookmark: Texte40]     
	[bookmark: Texte44]     
	[bookmark: Texte48]     

	Verified
	[bookmark: Texte29]     
	[bookmark: Texte33]     
	[bookmark: Texte37]     
	[bookmark: Texte41]     
	[bookmark: Texte45]     
	[bookmark: Texte49]     

	Approved
	[bookmark: Texte30]     
	[bookmark: Texte34]     
	[bookmark: Texte38]     
	[bookmark: Texte42]     
	[bookmark: Texte46]     
	[bookmark: Texte50]     



	COMMODITY CODE
Option code Ends connection
	[bookmark: Texte52]     
	[bookmark: Texte53]     
	[bookmark: Texte54]     

	
	     
	[bookmark: Texte56]     
	[bookmark: Texte57]     

	Valve type
	Manual 
	Valve tag number
	[bookmark: Texte66]     

	Service Class (GS EP PVV 142)
	A |_| B |_| C |_| D |_| E |_|
	Total Piping Class / 
Piping class rating
	[bookmark: Texte67]     

	Pressure class
(ASME B16.34/API 6A)
	[bookmark: Texte58]     
	Corrosion allowance - mm
	     

	Nominal Size
	[bookmark: Texte59]     
	Class pressure / temperature
	[bookmark: Texte68]     

	Bore (mm)
	[bookmark: Texte60]     
	
	[bookmark: Texte69]     

	Internal bore
	[bookmark: Texte61]     
	Min/Max design pressure - bar
	[bookmark: Texte70]     
	     

	Above ground / Underground
	[bookmark: Texte62]     
	Min/Max design temperature °C
	[bookmark: Texte71]     
	     

	Insulation
	[bookmark: Texte63]     
	Min/Max operating temp. °C
	[bookmark: Texte72]     
	     

	     
	     
	Min depressurisation temperature °C
	     

	Design
	Main Fluids
	     

	Construction standard
	[bookmark: Texte80]     
	Solid particles in fluid 
(note 6 of table 7.6.b, section 7.6 of GS EP PVV 142)
	     

	Construction type
	[bookmark: Texte81]     
	H2S/CO2 max content (%)
	     
	     

	Fire safe
	     
	Methanol max content
	     

	Floating or 
trunnion mounted ball
	     
	Chemical treatment of line
	[bookmark: Texte78]     

	Extended stem
	     
	     
	[bookmark: Texte79]     

	Operation (gear/wrench)
	     
	     
	     

	End connections:
	
	Metallic materials

	· Flanges
	     
	Body
	     

	· Pup  piece
	     
	Ball
	     

	· Transition piece
	     
	Stem
	     

	· Hub connectors
	     
	Seat spring/Seat washer
	     

	End to end dimensions
	     
	Seat holder
	     

	Flanges facing finish or grooves facing finish
	     
	Bolting 
(section 8.6.3 of GS EP PVV 142)
	[bookmark: Texte96]     

	By Pass
	     
	Weld Overlay
	[bookmark: Texte97]     

	Stem position (Vertical/Horizontal)
	     
	Internal seals materials 
(as per table 7.6.b of GS EP PVV 142)

	Flow axes  (Vertical/Horizontal)
	     
	Seat Inserts (note 1)
	[bookmark: Texte129]     

	Drains, vents 
(table 7.5 of GS EP PVV 142)
	     
	Dynamic seat seals
	[bookmark: Texte130]     

	Sealant injection on seats 
(table 7.5 of GS EP PVV 142)
	     
	Dynamic stem seals
	[bookmark: Texte131]     

	Sealant injection on stem
(table 7.5 of GS EP PVV 142)
	     
	Static seals
	[bookmark: Texte132]     

	Lifting Lugs
	     
	Fire safe graphite back-up seals
	     

	Valve Support
	     
	     
	     

	Lock Open / Lock Close
	     
	     
	     

	P.E.D
	Delivery requirements

	FLUID:	Liquid	|_|	Gas	|_|
	Dangerous	|_|	Not dangerous	|_|
	Non destructive tests
	[bookmark: Texte98]     

	Category
	     
	Pressure test certificates
	     

	Module
	     
	Material certificates
	     

	     
	     
	Fire Safe certificate
	     

	     
	     
	Marking
	     

	     
	     
	Calculation note of body thickness 
(section 8.1 of GS EP PVV 142)
	[bookmark: Texte99]     

	     
	     
	Bolting Calculation note 
(section 8.7.1 of GS EP PVV 142)
	[bookmark: Texte100]     

	     
	     
	External coating
	[bookmark: Texte101]     

	     
	     
	Colour code
	[bookmark: Texte102]     

	Notes:
Note 1: Elastomeric material is prohibited
[bookmark: Texte123]     



This document is the property of Total. It must not be stored, reproduced or disclosed to others without written authorisation from the Company.
DS_EP_PVV_142_00p2
This document is the property of Total. It must not be stored, reproduced or disclosed to others without written authorisation from the Company.
DS_EP_PVV_142_00p2	Page 2/2
image1.png




oleObject1.bin
2/1



[image: image1.png]





Image dans CR-specimenrev1.doc

Image dans CR-specimenrev1.doc




oleObject2.bin
2/1



[image: image1.png]





Image dans CR-specimenrev1.doc

Image dans CR-specimenrev1.doc




